NAXIS1 = 108520 Table of graphics options: Select the desired graphics option (1) X vs. Y (2) Sx-curve vs. x-axis (A) X (H) PMTYA (3) Sy-curve vs. y-axis (B) Y (I) PMTYB (4) Rx vs. X (C) Sx-curve (J) [PMTXA + PMTXB] (5) Ry vs. Y (D) Sy-curve (K) [PMTYA + PMTYB] (6) x-position vs. time (E) Time (L) PMTsum (7) y-position vs. time (F) PMTXA (M) Theta A (8) Sx vs. time (G) PMTXB (N) Theta B (9) Sy vs. time (10) [PMTXA + PMTXB] vs. time (11) [PMTYA + PMTYB] vs. time (Z) I/O Parameters (12) PMTsum vs. time (ZX) co-added X s-curves (UX) FESAVG_X (ZY) co_added Y s-curves (UY) FESAVG_Y (XA) co_added XA pmt counts (XB) co_added XB pmt counts (YA) co_added YA pmt counts (YB) co_added YB pmt counts (XS) co_added XA,B pmt counts (YS) co_added YA,B pmt counts Your choice (^Z for help) ->